; SPAAAX9.INF 
; 
; Copyright (C) 2009 TallyGenicom, LP. All rights reserved. 
; Microsoft PCL6 Driver for Windows 95/98/Me. 
; 
 
[Version] 
Signature="$Windows 95$" 
Class=Printer 
InfVersion=9.1 
Provider=%SP% 
DriverVer=12/21/2009,1.0.24 
 
[Manufacturer] 
%SP%=SP 
 
[SP] 
SHARP DX-B450P PCL6=SPAAAX.XPI,LPTENUM\SharpDX-B450P6430 
SHARP DX-B450P PCL6=SPAAAX.XPI,USBPRINT\SharpDX-B450P6430 
SHARP DX-B350P PCL6=SPAAAX.XPI,LPTENUM\SharpDX-B350P1031 
SHARP DX-B350P PCL6=SPAAAX.XPI,USBPRINT\SharpDX-B350P1031 
 
[SPAAAX.XPI] 
Copyfiles=SPFiles,AAAFiles,MONITOR 
DataSection=SPData 
PortMonitor=usbmon.dll,usbmon.dll 
 
[MONITOR] 
usbmon.dll,,,16 
 
[SourceDisksNames] 
1=%DiskID%,,0 
 
[DestinationDirs] 
DefaultDestDir=11 
 
[SourceDisksFiles] 
SPAAAXD.DRV=1 
SPAAAXG.DLL=1 
SPAAAXEN.DLL=1 
SPAAAXEN.CHM=1 
SPAAAX.XPI=1 
SPAAAXEN.INI=1 
SPAAAXW.EXE=1 
SPAAAXP.EXE=1 
SPAAAH3.DLL=1 
SPAAAX9.VER=1 
SPAAAX.CAP=1 
TGHLP16.DLL=1 
TGHLP32.DLL=1 
USBMON.DLL=1 
 
[SPFiles] 
SPAAAXD.DRV 
SPAAAXG.DLL 
SPAAAXEN.DLL 
SPAAAXEN.CHM 
SPAAAXW.EXE 
SPAAAXP.EXE 
SPAAAH3.DLL 
SPAAAX9.VER 
SPAAAX.CAP 
TGHLP16.DLL 
TGHLP32.DLL 
 
[AAAFiles] 
SPAAAX.XPI 
SPAAAXEN.INI 
 
[SPData] 
DriverFile=SPAAAXD.DRV 
HelpFile=SPAAAXEN.CHM 
 
[Strings] 
SP="Sharp" 
DiskID="Sharp DX-B350P/B450P Printer Installation Disk" 
DrvOSVersion="0" 
EnableOption="0" 
 
